0
control 0
5
9
Step 1: Select a source.
5
20
300
80

400

1

1


control 1
1
10
Confirm
255
105
50
20


400
Rotate theis source to a surfbin




control 2
2
10

130
105
40
20
1

400
press ENTER to change or use the buttons below




control 3
1
10
<
35
135
55
20
1

400
Select a previos source




control 4
1
10
>
100
135
55
20
1

400
Select the next source




control 5
4
8

20
185
120
18
1

Rotate from center, top left, top right or bottom





control 6
0
10
Rotate this source
5
110
115
20


400
Confirm




control 7
0
10
Instructions
15
5
75
15


400
Confirm




control 8
0
10
Rotation point
5
165
120
20
1

400





